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Description automatically generated]
This is an example of this technology, Note: NSTA do not endorse or recommend specific technologies. 
This is an extract from the Vendors website page for this product, the link for the full webpage is below for further information. 

Link: Electric submersible pump control - Artificial lift (Oil and gas) | ABB
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Electric submersible pump control with the ACS880 drives

‘Well conditions and oilinflow are changing over time and therefore an electric submersible pump.

(£SP) system needs to be tuned accordingly for optimized oflproduction. ACSB80 drives includea  Ar€ You looking for s

built-in control software that keeps ESP under control in changing well conditions and lets it run information?
relisoly day after day.
« contactus
Key benefits Share this page
+ Backspin detection without additional and costly measurements. I] m u

+ Save energy without compromizing on motor performance
+ Reduced motor temperature and longer lifetime

+ Gas underload ride through

+ Reliable start

+ Flow rate calculation and supervision without external flow sensors

Links and downloads

program firmuare manual  program firmware manual
~ Drive composer version




